**Instructions for Getting Started,   
by Shamoon Irshad, August 31 2017.**

The basic idea is talked about in the .ppt presentation file. See also the last section in Ali’s instruction guide .docx file

The Crazyflie’s general information and tools are available at the developer’s wiki: <https://wiki.bitcraze.io/doc:crazyflie:index>

From the wiki you will need to download and install and set-up the Bitcraze Virtual Machine VM for linux based development. The original firmware will be present inside the VM. See <https://wiki.bitcraze.io/projects:virtualmachine:index>

Additionally, download the latest version of the C++ boost library from <http://www.boost.org/users/download/> . Unzip the boost library at some location in your VM and modify the boost library path in the Makefile to your boost library path.

Request a purchase for the Crazyflie Radio USB Dongle. This will facilitate the flashing/firmware uploading.